;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Diameter##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Description##OTHER##;Type##Other##
ROBUST RING Ceiling/Wall LED ANTRACIT_300638;120;1.6;3000;787;Polycarbonate - Fagerhult - Opal;260;787;3000;3000;65;58;Anthracite grey;Aluminium - Fagerhult - Anthracite Grey;7320043009918;300638;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;0
ROBUST RING Ceiling/Wall LED WHITE_300639;120;1.6;3000;787;Polycarbonate - Fagerhult - Opal;260;787;3000;3000;65;58;White;Aluminium - Fagerhult - White;7320043009925;300639;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;0
ROBUST RING Ceiling/Wall LED BLACK_300640;120;1.6;3000;787;Polycarbonate - Fagerhult - Opal;260;787;3000;3000;65;58;Black;Aluminium - Fagerhult - Black;7320043009932;300640;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;0
ROBUST RING Ceiling/Wall LED GREY_300641;120;1.6;3000;787;Polycarbonate - Fagerhult - Opal;260;787;3000;3000;65;58;Alu Grey;Aluminium - Fagerhult - Alugrey;7320043009949;300641;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;0
ROBUST EYE Ceiling/Wall LED ANTRACIT_301630;120;1.7;3000;392;Polycarbonate - Fagerhult - Opal;260;392;3000;3000;65;29;Anthracite grey;Aluminium - Fagerhult - Anthracite Grey;7320046923044;301630;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;1
ROBUST EYE Ceiling/Wall LED WHITE_301631;120;1.7;3000;392;Polycarbonate - Fagerhult - Opal;260;392;3000;3000;65;29;White;Aluminium - Fagerhult - White;7320046923051;301631;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;1
ROBUST EYE Ceiling/Wall LED BLACK_301632;120;1.7;3000;392;Polycarbonate - Fagerhult - Opal;260;392;3000;3000;65;29;Black;Aluminium - Fagerhult - Black;7320046923099;301632;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;1
ROBUST EYE Ceiling/Wall LED GREY_301633;120;1.7;3000;392;Polycarbonate - Fagerhult - Opal;260;392;3000;3000;65;29;Alu Grey;Aluminium - Fagerhult - Alugrey;7320046923112;301633;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;1
ROBUST GRILL Ceiling/Wall LED ANTRACIT_301634;120;1.5;3000;671;Polycarbonate - Fagerhult - Opal;260;671;3000;3000;65;50;Anthracite grey;Aluminium - Fagerhult - Anthracite Grey;7320046923129;301634;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;2
ROBUST GRILL Ceiling/Wall LED WHITE_301635;120;1.5;3000;671;Polycarbonate - Fagerhult - Opal;260;671;3000;3000;65;50;White;Aluminium - Fagerhult - White;7320046923167;301635;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;2
ROBUST GRILL Ceiling/Wall LED BLACK_301636;120;1.5;3000;671;Polycarbonate - Fagerhult - Opal;260;671;3000;3000;65;50;Black;Aluminium - Fagerhult - Black;7320046923174;301636;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;2
ROBUST GRILL Ceiling/Wall LED GREY_301637;120;1.5;3000;671;Polycarbonate - Fagerhult - Opal;260;671;3000;3000;65;50;Alu Grey;Aluminium - Fagerhult - Alugrey;7320046923204;301637;13.5;Wall and ceiling luminaire for entrances and walkways. Available in three different styles.;2
