;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Lighting Control##OTHER##;Type End Cap##OTHER##
ALLFIVE 600 ON/OFF HL PRISM 830_33300-20005;130;1.3;3000;2964;Acrylic - Fagerhult - Clear Prismatic;621;2964;3000;3000;44;49;136;White;Aluzinc - Fagerhult - White;7316911137692;33300-20005;22;22;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 ON/OFF LL PRISM 830_33301-20003;130;2.2;3000;4667;Acrylic - Fagerhult - Clear Prismatic;1145;4667;3000;3000;44;49;158;White;Aluzinc - Fagerhult - White;7316911106001;33301-20003;30;30;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 ON/OFF LL PRISM 830_33301-20004;130;2.3;3000;4667;Acrylic - Fagerhult - Clear Prismatic;1145;4667;3000;3000;44;49;158;White;Aluzinc - Fagerhult - White;7316911137890;33301-20004;30;30;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 DALI LL PRISM 830_33301-20005;130;2.1;3000;4212;Acrylic - Fagerhult - Clear Prismatic;1145;4212;3000;3000;21;49;157;White;Aluzinc - Fagerhult - White;7316911137937;33301-20005;28.5;28.5;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;2;1
ALLFIVE 1200 DALI LL PRISM 830_33301-20006;130;2;3000;4212;Acrylic - Fagerhult - Clear Prismatic;1145;4212;3000;3000;44;49;161;White;Aluzinc - Fagerhult - White;7316911137975;33301-20006;27.5;27.5;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 ON/OFF LL PRISM 830_33301-20007;130;2.2;3000;4667;Acrylic - Fagerhult - Clear Prismatic;1145;4667;3000;3000;41;49;154;White;Aluzinc - Fagerhult - White;7316911138019;33301-20007;30;30;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;3;1
ALLFIVE 1200 ON/OFF LL PRISM 830_33301-20008;130;2.1;3000;4667;Acrylic - Fagerhult - Clear Prismatic;1145;4667;3000;3000;44;49;152;White;Aluzinc - Fagerhult - White;7316911138057;33301-20008;31;31;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 ON/OFF LL PRISM 840_33301-20009;130;2.2;4000;4801;Acrylic - Fagerhult - Clear Prismatic;1145;4801;4000;4000;44;49;162;White;Aluzinc - Fagerhult - White;7316911138095;33301-20009;30;30;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 DALI LL PRISM 840_33301-20012;130;2;4000;4333;Acrylic - Fagerhult - Clear Prismatic;1145;4333;4000;4000;44;49;165;White;Aluzinc - Fagerhult - White;7316911138217;33301-20012;27.5;27.5;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 ON/OFF LL PRISM 840_33301-20014;130;2.1;4000;4801;Acrylic - Fagerhult - Clear Prismatic;1145;4801;4000;4000;44;49;156;White;Aluzinc - Fagerhult - White;7316911138293;33301-20014;31;31;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 ON/OFF HL PRISM 830_33301-20015;130;2.2;3000;6026;Acrylic - Fagerhult - Clear Prismatic;1145;6026;3000;3000;44;49;157;White;Aluzinc - Fagerhult - White;7316911119285;33301-20015;38;38;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 ON/OFF HL PRISM 830_33301-20016;130;2.3;3000;6026;Acrylic - Fagerhult - Clear Prismatic;1145;6026;3000;3000;44;49;157;White;Aluzinc - Fagerhult - White;7316911138330;33301-20016;38;38;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 DALI HL PRISM 830_33301-20018;130;2;3000;5451;Acrylic - Fagerhult - Clear Prismatic;1145;5451;3000;3000;44;49;157;White;Aluzinc - Fagerhult - White;7316911138415;33301-20018;36;36;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 ON/OFF HL PRISM 840_33301-20021;130;2.2;4000;6200;Acrylic - Fagerhult - Clear Prismatic;1145;6200;4000;4000;44;49;162;White;Aluzinc - Fagerhult - White;7316911138491;33301-20021;38;38;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 DALI HL PRISM 840_33301-20024;130;2;4000;5608;Acrylic - Fagerhult - Clear Prismatic;1145;5608;4000;4000;44;49;165;White;Aluzinc - Fagerhult - White;7316911138613;33301-20024;36;36;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1200 ON/OFF HL PRISM 840_33301-20026;130;2.1;4000;6200;Acrylic - Fagerhult - Clear Prismatic;1145;6200;4000;4000;44;49;157;White;Aluzinc - Fagerhult - White;7316911138699;33301-20026;40;40;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1500 DALI HL PRISM 830_33302-20004;130;2.6;3000;7552;Acrylic - Fagerhult - Clear Prismatic;1513;7552;3000;3000;44;49;161;White;Aluzinc - Fagerhult - White;7316911138828;33302-20004;49.5;49.5;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
ALLFIVE 1500 DALI HL PRISM 840_33302-20010;130;2.6;4000;7770;Acrylic - Fagerhult - Clear Prismatic;1513;7770;4000;4000;44;49;166;White;Aluzinc - Fagerhult - White;7316911139061;33302-20010;49.5;49.5;AllFive;Surface mounted, cable wire, wire suspension or on a wall. Installation using the seal supplied with the luminaire provides protection classification IP 44. With wall mounting or installation without seals the luminaire is classified IP 40.;A universal luminaire, developed for industrial use with IP 44 to withstand moisture and mechanical stress. AllFive is just as suitable for garages and culverts as laundry rooms and kitchens.;min. 80;C;1;1;2
