;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##;Sensor##OTHER##
HERO 12KLM WIDE 4000K HTG_31501;307;7.3;4000;12068;498;12068;4000;4000;66;87;154;Black;Aluminium - Fagerhult - Black;7320046433574;31501;78;78;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 12KLM WIDE 4000K HTG_31501-461;307;7.3;4000;12068;498;12068;4000;4000;66;87;157;Black;Aluminium - Fagerhult - Black;7320046433598;31501-461;80.5;80.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 12KLM WIDE 4000K HTG_31501-526;307;7.3;4000;12068;589;12068;4000;4000;65;102;154;Black;Aluminium - Fagerhult - Black;7320047242953;31501-526;82;82;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;1
HERO 16KLM WIDE 4000K HTG_31502;307;7.3;4000;16034;498;16034;4000;4000;66;87;160;Black;Aluminium - Fagerhult - Black;7320046433680;31502;100;100;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 16KLM WIDE 4000K HTG_31502-461;307;7.3;4000;16034;498;16034;4000;4000;66;87;162;Black;Aluminium - Fagerhult - Black;7320046433734;31502-461;103.5;103.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 16KLM WIDE 4000K HTG_31502-526;307;7.3;4000;16034;589;16034;4000;4000;65;102;159;Black;Aluminium - Fagerhult - Black;7320047242977;31502-526;105.5;105.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 20KLM WIDE 4000K HTG_31505;307;7.3;4000;19723;498;19723;4000;4000;66;87;151;Black;Aluminium - Fagerhult - Black;7320046433895;31505;131;131;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 20KLM WIDE 4000K HTG_31505-461;307;7.3;4000;19723;498;19723;4000;4000;66;87;153;Black;Aluminium - Fagerhult - Black;7320046433949;31505-461;135;135;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 20KLM WIDE 4000K HTG_31505-526;307;7.3;4000;19723;589;19723;4000;4000;65;102;151;Black;Aluminium - Fagerhult - Black;7320047243035;31505-526;136;136;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 12KLM WIDE 4000K PMMA_31511;307;7.3;4000;12032;498;12032;4000;4000;66;87;154;Black;Aluminium - Fagerhult - Black;7320046433604;31511;78;78;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 12KLM WIDE 4000K PMMA_31511-461;307;7.3;4000;12032;498;12032;4000;4000;66;87;156;Black;Aluminium - Fagerhult - Black;7320046433659;31511-461;80.5;80.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 12KLM WIDE 4000K PMMA_31511-526;307;7.3;4000;12032;589;12032;4000;4000;65;102;153;Black;Aluminium - Fagerhult - Black;7320047242960;31511-526;82;82;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;1
HERO 16KLM WIDE 4000K PMMA_31512;307;7.3;4000;15986;498;15986;4000;4000;66;87;159;Black;Aluminium - Fagerhult - Black;7320046433741;31512;100;100;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 16KLM WIDE 4000K PMMA_31512-461;307;7.3;4000;15986;498;15986;4000;4000;66;87;161;Black;Aluminium - Fagerhult - Black;7320046433765;31512-461;103.5;103.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 16KLM WIDE 4000K PMMA_31512-526;307;7.3;4000;15986;589;15986;4000;4000;65;102;159;Black;Aluminium - Fagerhult - Black;7320047242984;31512-526;105.5;105.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 20KLM WIDE 4000K PMMA_31515;307;7.3;4000;19664;498;19664;4000;4000;66;87;151;Black;Aluminium - Fagerhult - Black;7320046433963;31515;131;131;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 20KLM WIDE 4000K PMMA_31515-461;307;7.3;4000;19664;498;19664;4000;4000;66;87;152;Black;Aluminium - Fagerhult - Black;7320046433987;31515-461;135;135;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 20KLM WIDE 4000K PMMA_31515-526;307;7.3;4000;19664;589;19664;4000;4000;65;102;151;Black;Aluminium - Fagerhult - Black;7320047243042;31515-526;136;136;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 12KLM WIDE HTG FROSTED 840_31560;307;7.3;4000;11465;498;11465;4000;4000;66;87;140;Black;Aluminium - Fagerhult - Black;7320047788789;31560;82;82;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 12KLM WIDE HTG FROSTED 840_31560-461;307;7.300;4000;11465;498;11465;4000;4000;66;87;142;Black;Aluminium - Fagerhult - Black;7320047788796;31560-461;84.5;84.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 16KLM WIDE  HTG FROSTED 840_31561;307;7.3;4000;15232;498;15232;4000;4000;66;87;144;Black;Aluminium - Fagerhult - Black;7320047788802;31561;106;106;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 16KLM WIDE  HTG FROSTED 840_31561-461;307;7.3;4000;15232;498;15232;4000;4000;66;87;145;Black;Aluminium - Fagerhult - Black;7320047788826;31561-461;110.5;110.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 20KLM WIDE HTG FROSTED 840_31562;307;7.3;4000;18737;498;18737;4000;4000;66;87;141;Black;Aluminium - Fagerhult - Black;7320047788833;31562;133;133;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 20KLM WIDE HTG FROSTED 840_31562-461;307;7.3;4000;18737;498;18737;4000;4000;66;87;143;Black;Aluminium - Fagerhult - Black;7320047788857;31562-461;138;138;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 12KLM WIDE 4000K HTG_31501-579;307;7.300;4000;12068;589;12068;4000;4000;65;102;154;Black;Aluminium - Fagerhult - Black;7316912758056;31501-579;82;82;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;1
HERO 16KLM WIDE 4000K HTG_31502-579;307;7.300;4000;16034;589;16034;4000;4000;65;102;159;Black;Aluminium - Fagerhult - Black;7316912758094;31502-579;105.5;105.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 20KLM WIDE 4000K HTG_31505-579;307;7.300;4000;19723;589;19723;4000;4000;65;102;151;Black;Aluminium - Fagerhult - Black;7316912758131;31505-579;136;136;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 12KLM WIDE 4000K PMMA_31511-579;307;7.300;4000;12032;589;12032;4000;4000;65;102;153;Black;Aluminium - Fagerhult - Black;7316912758087;31511-579;82;82;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;1
HERO 16KLM WIDE 4000K PMMA_31512-579;307;7.300;4000;15986;589;15986;4000;4000;65;102;159;Black;Aluminium - Fagerhult - Black;7316912758100;31512-579;105.5;105.5;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 20KLM WIDE 4000K PMMA_31515-579;307;7.300;4000;19664;589;19664;4000;4000;65;102;151;Black;Aluminium - Fagerhult - Black;7316912758148;31515-579;136;136;Hero Wide Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
