;Diameter##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
KASKAD WW REC 95 LL 927 CRI 98 WHITE_76594;110;0,4;2700;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76594.IES;Kaskad Wallwasher;aluminium;648;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";648;2700;2700;44;100;52;Standard;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76594;12;98
KASKAD WW REC 95 HL 927 CRI 98 WHITE_76595;110;0,4;2700;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76595.IES;Kaskad Wallwasher;aluminium;1133;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";1133;2700;2700;44;100;57;Standard;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76595;20;98
KASKAD WW REC 95 LL 930 WHITE_76596;110;0,4;3000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76596.IES;Kaskad Wallwasher;aluminium;772;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";772;3000;3000;44;100;62;Standard;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76596;12;90
KASKAD WW REC 95 HL 930 WHITE_76597;110;0,4;3000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76597.IES;Kaskad Wallwasher;aluminium;1349;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";1349;3000;3000;44;100;68;Standard;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76597;20;90
KASKAD WW REC 95 LL 940 WHITE_76598;110;0,4;4000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76598.IES;Kaskad Wallwasher;aluminium;772;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";772;4000;4000;44;100;62;Standard;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76598;12;90
KASKAD WW REC 95 HL 940 WHITE_76599;110;0,4;4000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76599.IES;Kaskad Wallwasher;aluminium;1349;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";1349;4000;4000;44;100;68;Standard;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76599;20;90
KASKAD WW REC 95 LL 927 CRI 98 WHITE_76594-3;110;0,4;2700;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76594-3.IES;Kaskad Wallwasher;aluminium;648;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";648;2700;2700;44;100;52;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76594-3;12;98
KASKAD WW REC 95 LL 927 CRI 98 WHITE_76594-402;110;0,4;2700;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76594-402.IES;Kaskad Wallwasher;aluminium;648;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";648;2700;2700;44;100;52;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76594-402;12;98
KASKAD WW REC 95 HL 927 CRI 98 WHITE_76595-3;110;0,4;2700;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76595-3.IES;Kaskad Wallwasher;aluminium;1133;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";1133;2700;2700;44;100;57;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76595-3;20;98
KASKAD WW REC 95 HL 927 CRI 98 WHITE_76595-402;110;0,4;2700;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76595-402.IES;Kaskad Wallwasher;aluminium;1133;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";1133;2700;2700;44;100;57;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76595-402;20;98
KASKAD WW REC 95 LL 930 WHITE_76596-3;110;0,4;3000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76596-3.IES;Kaskad Wallwasher;aluminium;772;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";772;3000;3000;44;100;62;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76596-3;12;90
KASKAD WW REC 95 LL 930 WHITE_76596-402;110;0,4;3000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76596-402.IES;Kaskad Wallwasher;aluminium;772;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";772;3000;3000;44;100;62;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76596-402;12;90
KASKAD WW REC 95 HL 930 WHITE_76597-3;110;0,4;3000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76597-3.IES;Kaskad Wallwasher;aluminium;1349;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";1349;3000;3000;44;100;68;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76597-3;20;90
KASKAD WW REC 95 HL 930 WHITE_76597-402;110;0,4;3000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76597-402.IES;Kaskad Wallwasher;aluminium;1349;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";1349;3000;3000;44;100;68;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76597-402;20;90
KASKAD WW REC 95 LL 940 WHITE_76598-3;110;0,4;4000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76598-3.IES;Kaskad Wallwasher;aluminium;772;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";772;4000;4000;44;100;62;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76598-3;12;90
KASKAD WW REC 95 LL 940 WHITE_76598-402;110;0,4;4000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76598-402.IES;Kaskad Wallwasher;aluminium;772;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";772;4000;4000;44;100;62;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76598-402;12;90
KASKAD WW REC 95 HL 940 WHITE_76599-3;110;0,4;4000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76599-3.IES;Kaskad Wallwasher;aluminium;1349;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";1349;4000;4000;44;100;68;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76599-3;20;90
KASKAD WW REC 95 HL 940 WHITE_76599-402;110;0,4;4000;D 110 mm + H 100 mm;Cirle;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium.;76599-402.IES;Kaskad Wallwasher;aluminium;1349;Fagerhult_Frosted_glass;Ceiling;Recessed ;"A small, recessed downlight with asymmetric light distribution in three colour temperatures and two outputs for illuminating vertical surfaces.
";1349;4000;4000;44;100;68;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Wallwasher;76599-402;20;90
