;Diameter##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Description##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##;Optic Type##Other##
KASKAD FLEX REC 95 927 CRI 98 WHITE_76600;110;0,4;2700;D 110 mm + H 95 mm;Cirle;"A small, recessed downlight in three colour temperatures. The tilting and rotating Kaskad Flex lets you cast light exactly where you want.
";Kaskad Flex;aluminium;827;Fagerhult_Frosted_glass;Ceiling;Recessed ;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium. ;20;95;63;Standard;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Flex;76600;13;98;Kaskad flex head : 2700K
KASKAD FLEX REC 95 930 WHITE_76602;110;0,4;3000;D 110 mm + H 95 mm;Cirle;"A small, recessed downlight in three colour temperatures. The tilting and rotating Kaskad Flex lets you cast light exactly where you want.
";Kaskad Flex;aluminium;951;Fagerhult_Frosted_glass;Ceiling;Recessed ;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium. ;20;95;72;Standard;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Flex;76602;13;90;Kaskad flex head : 3000K
KASKAD FLEX REC 95 940 WHITE_76604;110;0,4;4000;D 110 mm + H 95 mm;Cirle;"A small, recessed downlight in three colour temperatures. The tilting and rotating Kaskad Flex lets you cast light exactly where you want.
";Kaskad Flex;aluminium;1030;Fagerhult_Frosted_glass;Ceiling;Recessed ;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium. ;20;95;78;Standard;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Flex;76604;13;90;Kaskad flex head : 4000K
KASKAD FLEX REC 95 927 CRI 98 WHITE_76600-3;110;0,4;2700;D 110 mm + H 95 mm;Cirle;"A small, recessed downlight in three colour temperatures. The tilting and rotating Kaskad Flex lets you cast light exactly where you want.
";Kaskad Flex;aluminium;827;Fagerhult_Frosted_glass;Ceiling;Recessed ;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium. ;20;95;63;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Flex;76600-3;13;98;Kaskad flex head : 2700K
KASKAD FLEX REC 95 927 CRI 98 WHITE_76600-402;110;0,4;2700;D 110 mm + H 95 mm;Cirle;"A small, recessed downlight in three colour temperatures. The tilting and rotating Kaskad Flex lets you cast light exactly where you want.
";Kaskad Flex;aluminium;827;Fagerhult_Frosted_glass;Ceiling;Recessed ;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium. ;20;95;63;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Flex;76600-402;13;98;Kaskad flex head : 2700K
KASKAD FLEX REC 95 930 WHITE_76602-3;110;0,4;3000;D 110 mm + H 95 mm;Cirle;"A small, recessed downlight in three colour temperatures. The tilting and rotating Kaskad Flex lets you cast light exactly where you want.
";Kaskad Flex;aluminium;951;Fagerhult_Frosted_glass;Ceiling;Recessed ;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium. ;20;95;72;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Flex;76602-3;13;90;Kaskad flex head : 3000K
KASKAD FLEX REC 95 930 WHITE_76602-402;110;0,4;3000;D 110 mm + H 95 mm;Cirle;"A small, recessed downlight in three colour temperatures. The tilting and rotating Kaskad Flex lets you cast light exactly where you want.
";Kaskad Flex;aluminium;951;Fagerhult_Frosted_glass;Ceiling;Recessed ;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium. ;20;95;72;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Flex;76602-402;13;90;Kaskad flex head : 3000K
KASKAD FLEX REC 95 940 WHITE_76604-3;110;0,4;4000;D 110 mm + H 95 mm;Cirle;"A small, recessed downlight in three colour temperatures. The tilting and rotating Kaskad Flex lets you cast light exactly where you want.
";Kaskad Flex;aluminium;1030;Fagerhult_Frosted_glass;Ceiling;Recessed ;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium. ;20;95;78;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Flex;76604-3;13;90;Kaskad flex head : 4000K
KASKAD FLEX REC 95 940 WHITE_76604-402;110;0,4;4000;D 110 mm + H 95 mm;Cirle;"A small, recessed downlight in three colour temperatures. The tilting and rotating Kaskad Flex lets you cast light exactly where you want.
";Kaskad Flex;aluminium;1030;Fagerhult_Frosted_glass;Ceiling;Recessed ;Luminaire body and visible edge ring of sheet steel in white (RAL 9016) structured enamel. Heatsink in black enamelled aluminium. ;20;95;78;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7,32005E+12;Kaskad Flex;76604-402;13;90;Kaskad flex head : 4000K
