;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##
NOVE G2 D360 830_59200-495;1.3;3000;1679;Acrylic - Fagerhult - Opal;1679;3000;3000;40;73;120;White;Steel - Fagerhult - White;7316912944794;59200-495;14;14;360;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;1
NOVE G2 D360 840_59201-495;1.3;4000;1775;Acrylic - Fagerhult - Opal;1775;4000;4000;40;73;127;White;Steel - Fagerhult - White;7316912944817;59201-495;14;14;360;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;1
NOVE G2 D420 830_59202-495;1.6;3000;2764;Acrylic - Fagerhult - Opal;2764;3000;3000;40;73;124;White;Steel - Fagerhult - White;7316912944831;59202-495;22;22;420;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;1
NOVE G2 D420 840_59203-495;1.6;4000;2922;Acrylic - Fagerhult - Opal;2922;4000;4000;40;73;131;White;Steel - Fagerhult - White;7316912944855;59203-495;22;22;420;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;1
NOVE G2 D520 830_59204-495;2.5;3000;4498;Acrylic - Fagerhult - Opal;4498;3000;3000;40;73;115;White;Steel - Fagerhult - White;7316912944879;59204-495;39;39;520;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;1
NOVE G2 D520 840_59205-495;2.5;4000;4755;Acrylic - Fagerhult - Opal;4755;4000;4000;40;73;112;White;Steel - Fagerhult - White;7316912944893;59205-495;39;39;520;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;1
NOVE G2 D360 830 DECOR WHITE_59206-495;1.7;3000;1588;Acrylic - Fagerhult - Opal;1588;3000;3000;40;73;113;White;Steel - Fagerhult - White;7316912944916;59206-495;14;14;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D360 840 DECOR WHITE_59207-495;1.7;4000;1679;Acrylic - Fagerhult - Opal;1679;4000;4000;40;73;120;White;Steel - Fagerhult - White;7316912944930;59207-495;14;14;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D420 830 DECOR WHITE_59208-495;2.0;3000;2615;Acrylic - Fagerhult - Opal;2615;3000;3000;40;73;118;White;Steel - Fagerhult - White;7316912944954;59208-495;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D420 840 DECOR WHITE_59209-495;2.0;4000;2764;Acrylic - Fagerhult - Opal;2764;4000;4000;40;73;124;White;Steel - Fagerhult - White;7316912944978;59209-495;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D520 830 DECOR WHITE_59210-495;3.1;3000;4255;Acrylic - Fagerhult - Opal;4255;3000;3000;40;73;109;White;Steel - Fagerhult - White;7316912944992;59210-495;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D520 840 DECOR WHITE_59211-495;3.1;4000;4498;Acrylic - Fagerhult - Opal;4498;4000;4000;40;73;115;White;Steel - Fagerhult - White;7316912945012;59211-495;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D360 830 DECOR SAND_59212-495;1.7;3000;1511;Acrylic - Fagerhult - Opal;1511;3000;3000;40;73;108;Sand;Steel - Fagerhult - Sand;7316912945036;59212-495;14;14;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D360 840 DECOR SAND_59213-495;1.7;4000;1598;Acrylic - Fagerhult - Opal;1598;4000;4000;40;73;114;Sand;Steel - Fagerhult - Sand;7316912945050;59213-495;14;14;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D420 830 DECOR SAND_59214-495;2.0;3000;2488;Acrylic - Fagerhult - Opal;2488;3000;3000;40;73;112;Sand;Steel - Fagerhult - Sand;7316912945074;59214-495;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D420 840 DECOR SAND_59215-495;2.0;4000;2630;Acrylic - Fagerhult - Opal;2630;4000;4000;40;73;118;Sand;Steel - Fagerhult - Sand;7316912945098;59215-495;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D520 830 DECOR SAND_59216-495;3.1;3000;4048;Acrylic - Fagerhult - Opal;4048;3000;3000;40;73;104;Sand;Steel - Fagerhult - Sand;7316912945111;59216-495;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D520 840 DECOR SAND_59217-495;3.1;4000;4280;Acrylic - Fagerhult - Opal;4280;4000;4000;40;73;110;Sand;Steel - Fagerhult - Sand;7316912945135;59217-495;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D360 830 DECOR AZURITE_59218-495;1.7;3000;1478;Acrylic - Fagerhult - Opal;1478;3000;3000;40;73;106;Azurite;Steel - Fagerhult - Azurite;7316912945159;59218-495;14;14;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D360 840 DECOR AZURITE_59219-495;1.7;4000;1562;Acrylic - Fagerhult - Opal;1562;4000;4000;40;73;112;Azurite;Steel - Fagerhult - Azurite;7316912945173;59219-495;14;14;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D420 830 DECOR AZURITE_59220-495;2.0;3000;2433;Acrylic - Fagerhult - Opal;2433;3000;3000;40;73;109;Azurite;Steel - Fagerhult - Azurite;7316912945197;59220-495;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D420 840 DECOR AZURITE_59221-495;2.0;4000;2571;Acrylic - Fagerhult - Opal;2571;4000;4000;40;73;116;Azurite;Steel - Fagerhult - Azurite;7316912945210;59221-495;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D520 830 DECOR AZURITE_59222-495;3.1;3000;3958;Acrylic - Fagerhult - Opal;3958;3000;3000;40;73;101;Azurite;Steel - Fagerhult - Azurite;7316912945234;59222-495;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D520 840 DECOR AZURITE_59223-495;3.1;4000;4184;Acrylic - Fagerhult - Opal;4184;4000;4000;40;73;107;Azurite;Steel - Fagerhult - Azurite;7316912945258;59223-495;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D360 830_59200-402;1.3;3000;1679;Acrylic - Fagerhult - Opal;1679;3000;3000;40;73;125;White;Steel - Fagerhult - White;7316912944312;59200-402;13;13;360;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;1
NOVE G2 D360 840_59201-402;1.3;4000;1775;Acrylic - Fagerhult - Opal;1775;4000;4000;40;73;132;White;Steel - Fagerhult - White;7316912944336;59201-402;13;13;360;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;1
NOVE G2 D420 830_59202-402;1.6;3000;2764;Acrylic - Fagerhult - Opal;2764;3000;3000;40;73;127;White;Steel - Fagerhult - White;7316912944350;59202-402;22;22;420;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;1
NOVE G2 D420 840_59203-402;1.6;4000;2922;Acrylic - Fagerhult - Opal;2922;4000;4000;40;73;134;White;Steel - Fagerhult - White;7316912944374;59203-402;22;22;420;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;1
NOVE G2 D520 830_59204-402;2.5;3000;4498;Acrylic - Fagerhult - Opal;4498;3000;3000;40;73;117;White;Steel - Fagerhult - White;7316912944398;59204-402;39;39;520;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;1
NOVE G2 D520 840_59205-402;2.5;4000;4755;Acrylic - Fagerhult - Opal;4755;4000;4000;40;73;124;White;Steel - Fagerhult - White;7316912944411;59205-402;39;39;520;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;1
NOVE G2 D360 830 DECOR WHITE_59206-402;1.7;3000;1588;Acrylic - Fagerhult - Opal;1588;3000;3000;40;73;118;White;Steel - Fagerhult - White;7316912944435;59206-402;13;13;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D360 840 DECOR WHITE_59207-402;1.7;4000;1679;Acrylic - Fagerhult - Opal;1679;4000;4000;40;73;125;White;Steel - Fagerhult - White;7316912944459;59207-402;13;13;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D420 830 DECOR WHITE_59208-402;2.0;3000;2615;Acrylic - Fagerhult - Opal;2615;3000;3000;40;73;120;White;Steel - Fagerhult - White;7316912944473;59208-402;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D420 840 DECOR WHITE_59209-402;2.0;4000;2764;Acrylic - Fagerhult - Opal;2764;4000;4000;40;73;127;White;Steel - Fagerhult - White;7316912944497;59209-402;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D520 830 DECOR WHITE_59210-402;3.1;3000;4255;Acrylic - Fagerhult - Opal;4255;3000;3000;40;73;111;White;Steel - Fagerhult - White;7316912944510;59210-402;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D520 840 DECOR WHITE_59211-402;3.1;4000;4498;Acrylic - Fagerhult - Opal;4498;4000;4000;40;73;117;White;Steel - Fagerhult - White;7316912944534;59211-402;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D360 830 DECOR SAND_59212-402;1.7;3000;1511;Acrylic - Fagerhult - Opal;1511;3000;3000;40;73;112;Sand;Steel - Fagerhult - Sand;7316912944558;59212-402;13;13;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D360 840 DECOR SAND_59213-402;1.7;4000;1598;Acrylic - Fagerhult - Opal;1598;4000;4000;40;73;119;Sand;Steel - Fagerhult - Sand;7316912944572;59213-402;13;13;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D420 830 DECOR SAND_59214-402;2.0;3000;2488;Acrylic - Fagerhult - Opal;2488;3000;3000;40;73;114;Sand;Steel - Fagerhult - Sand;7316912944596;59214-402;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D420 840 DECOR SAND_59215-402;2.0;4000;2630;Acrylic - Fagerhult - Opal;2630;4000;4000;40;73;121;Sand;Steel - Fagerhult - Sand;7316912944619;59215-402;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D520 830 DECOR SAND_59216-402;3.1;3000;4048;Acrylic - Fagerhult - Opal;4048;3000;3000;40;73;105;Sand;Steel - Fagerhult - Sand;7316912944633;59216-402;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D520 840 DECOR SAND_59217-402;3.1;4000;4280;Acrylic - Fagerhult - Opal;4280;4000;4000;40;73;111;Sand;Steel - Fagerhult - Sand;7316912944657;59217-402;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D360 830 DECOR AZURITE_59218-402;1.7;3000;1478;Acrylic - Fagerhult - Opal;1478;3000;3000;40;73;110;Azurite;Steel - Fagerhult - Azurite;7316912944671;59218-402;13;13;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D360 840 DECOR AZURITE_59219-402;1.7;4000;1562;Acrylic - Fagerhult - Opal;1562;4000;4000;40;73;116;Azurite;Steel - Fagerhult - Azurite;7316912944695;59219-402;13;13;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D420 830 DECOR AZURITE_59220-402;2.0;3000;2433;Acrylic - Fagerhult - Opal;2433;3000;3000;40;73;112;Azurite;Steel - Fagerhult - Azurite;7316912944718;59220-402;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D420 840 DECOR AZURITE_59221-402;2.0;4000;2571;Acrylic - Fagerhult - Opal;2571;4000;4000;40;73;118;Azurite;Steel - Fagerhult - Azurite;7316912944732;59221-402;22;22;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D520 830 DECOR AZURITE_59222-402;3.1;3000;3958;Acrylic - Fagerhult - Opal;3958;3000;3000;40;73;103;Azurite;Steel - Fagerhult - Azurite;7316912944756;59222-402;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D520 840 DECOR AZURITE_59223-402;3.1;4000;4184;Acrylic - Fagerhult - Opal;4184;4000;4000;40;73;109;Azurite;Steel - Fagerhult - Azurite;7316912944770;59223-402;39;39;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D360 830_59200-569;1.3;3000;1679;Acrylic - Fagerhult - Opal;1679;3000;3000;40;73;114;White;Steel - Fagerhult - White;7316912963078;59200-569;15;15;360;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;1
NOVE G2 D360 840_59201-569;1.3;4000;1775;Acrylic - Fagerhult - Opal;1775;4000;4000;40;73;121;White;Steel - Fagerhult - White;7316912963085;59201-569;15;15;360;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;1
NOVE G2 D420 830_59202-569;1.6;3000;2764;Acrylic - Fagerhult - Opal;2764;3000;3000;40;73;120;White;Steel - Fagerhult - White;7316912963092;59202-569;23;23;420;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;1
NOVE G2 D420 840_59203-569;1.6;4000;2922;Acrylic - Fagerhult - Opal;2922;4000;4000;40;73;127;White;Steel - Fagerhult - White;7316912963108;59203-569;23;23;420;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;1
NOVE G2 D520 830_59204-569;2.5;3000;4498;Acrylic - Fagerhult - Opal;4498;3000;3000;40;73;113;White;Steel - Fagerhult - White;7316912963115;59204-569;40;40;520;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;1
NOVE G2 D520 840_59205-569;2.5;4000;4755;Acrylic - Fagerhult - Opal;4755;4000;4000;40;73;120;White;Steel - Fagerhult - White;7316912963122;59205-569;40;40;520;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;1
NOVE G2 D360 830 DECOR WHITE_59206-569;1.7;3000;1588;Acrylic - Fagerhult - Opal;1588;3000;3000;40;73;108;White;Steel - Fagerhult - White;7316912963276;59206-569;15;15;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D360 840 DECOR WHITE_59207-569;1.7;4000;1679;Acrylic - Fagerhult - Opal;1679;4000;4000;40;73;114;White;Steel - Fagerhult - White;7316912963290;59207-569;15;15;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D420 830 DECOR WHITE_59208-569;2.0;3000;2615;Acrylic - Fagerhult - Opal;2615;3000;3000;40;73;114;White;Steel - Fagerhult - White;7316912963313;59208-569;23;23;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D420 840 DECOR WHITE_59209-569;2.0;4000;2764;Acrylic - Fagerhult - Opal;2764;4000;4000;40;73;120;White;Steel - Fagerhult - White;7316912963337;59209-569;23;23;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D520 830 DECOR WHITE_59210-569;3.1;3000;4255;Acrylic - Fagerhult - Opal;4255;3000;3000;40;73;107;White;Steel - Fagerhult - White;7316912963351;59210-569;40;40;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D520 840 DECOR WHITE_59211-569;3.1;4000;4498;Acrylic - Fagerhult - Opal;4498;4000;4000;40;73;113;White;Steel - Fagerhult - White;7316912963375;59211-569;40;40;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D360 830 DECOR SAND_59212-569;1.7;3000;1511;Acrylic - Fagerhult - Opal;1511;3000;3000;40;73;103;Sand;Steel - Fagerhult - Sand;7316912963399;59212-569;15;15;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D360 840 DECOR SAND_59213-569;1.7;4000;1598;Acrylic - Fagerhult - Opal;1598;4000;4000;40;73;109;Sand;Steel - Fagerhult - Sand;7316912963412;59213-569;15;15;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D420 830 DECOR SAND_59214-569;2.0;3000;2488;Acrylic - Fagerhult - Opal;2488;3000;3000;40;73;108;Sand;Steel - Fagerhult - Sand;7316912963436;59214-569;23;23;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D420 840 DECOR SAND_59215-569;2.0;4000;2630;Acrylic - Fagerhult - Opal;2630;4000;4000;40;73;115;Sand;Steel - Fagerhult - Sand;7316912963450;59215-569;23;23;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D520 830 DECOR SAND_59216-569;3.1;3000;4048;Acrylic - Fagerhult - Opal;4048;3000;3000;40;73;102;Sand;Steel - Fagerhult - Sand;7316912963474;59216-569;40;40;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D520 840 DECOR SAND_59217-569;3.1;4000;4280;Acrylic - Fagerhult - Opal;4280;4000;4000;40;73;108;Sand;Steel - Fagerhult - Sand;7316912963498;59217-569;40;40;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D360 830 DECOR AZURITE_59218-569;1.7;3000;1478;Acrylic - Fagerhult - Opal;1478;3000;3000;40;73;101;Azurite;Steel - Fagerhult - Azurite;7316912963511;59218-569;15;15;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D360 840 DECOR AZURITE_59219-569;1.7;4000;1562;Acrylic - Fagerhult - Opal;1562;4000;4000;40;73;106;Azurite;Steel - Fagerhult - Azurite;7316912963535;59219-569;15;15;375;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D420 830 DECOR AZURITE_59220-569;2.0;3000;2433;Acrylic - Fagerhult - Opal;2433;3000;3000;40;73;106;Azurite;Steel - Fagerhult - Azurite;7316912963559;59220-569;23;23;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D420 840 DECOR AZURITE_59221-569;2.0;4000;2571;Acrylic - Fagerhult - Opal;2571;4000;4000;40;73;112;Azurite;Steel - Fagerhult - Azurite;7316912963573;59221-569;23;23;437;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
NOVE G2 D520 830 DECOR AZURITE_59222-569;3.1;3000;3958;Acrylic - Fagerhult - Opal;3958;3000;3000;40;73;101;Azurite;Steel - Fagerhult - Azurite;7316912963597;59222-569;40;40;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;C;1;2
NOVE G2 D520 840 DECOR AZURITE_59223-569;3.1;4000;4184;Acrylic - Fagerhult - Opal;4184;4000;4000;40;73;105;Azurite;Steel - Fagerhult - Azurite;7316912963610;59223-569;40;40;537;Nove;"For ceiling or wall mounting. </br>
Ø520?mm – three securing holes. </br>
Ø360/420?mm – two securing holes. </br>
Installation in ceilings with decor ring - IP44</br> Without decor ring - IP41</br>
Permanent wall mounting - IP40.";A decorative luminaire available in three sizes for ceiling or wall mounting in e.g. general areas, entrances and stairwells. The luminaire can be used with or without decor ring.;min. 80;B;1;2
