;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
PLEIAD G4 168 SURF DALI BLACK WIDE HL 830_72540-402;0.5;3000;3076;Aluminium - Fagerhult - Black;3076;3000;3000;20;154;115;White/Black;Aluminium - Fagerhult - White;7320047800801;72540-402;27;27;168;Pleiad G4 168 Surface mounted;Surface mounted installation. Installation section with two securing holes. See accessories for suspended installation.;Surface mounted downlights with integrated option for surface-mounted cable. Available with several reflector and light distribution options.;min. 80;E;1
PLEIAD G4 168 SURF DALI BLACK WIDE HL 840_72542-402;0.5;4000;3151;Aluminium - Fagerhult - Black;3151;4000;4000;20;154;118;White/Black;Aluminium - Fagerhult - White;7320047800887;72542-402;27;27;168;Pleiad G4 168 Surface mounted;Surface mounted installation. Installation section with two securing holes. See accessories for suspended installation.;Surface mounted downlights with integrated option for surface-mounted cable. Available with several reflector and light distribution options.;min. 80;E;1
PLEIAD G4 168 SURF DALI MATT WIDE HL 830_72566-402;0.5;3000;3860;Aluminium - Fagerhult - Alugrey;3860;3000;3000;20;154;145;White/alu;Aluminium - Fagerhult - White;7320047801808;72566-402;27;27;168;Pleiad G4 168 Surface mounted;Surface mounted installation. Installation section with two securing holes. See accessories for suspended installation.;Surface mounted downlights with integrated option for surface-mounted cable. Available with several reflector and light distribution options.;min. 80;E;1
PLEIAD G4 168 SURF DALI MATT WIDE HL 840_72568-402;0.5;4000;3954;Aluminium - Fagerhult - Alugrey;3954;4000;4000;20;154;148;White/alu;Aluminium - Fagerhult - White;7320047801884;72568-402;27;27;168;Pleiad G4 168 Surface mounted;Surface mounted installation. Installation section with two securing holes. See accessories for suspended installation.;Surface mounted downlights with integrated option for surface-mounted cable. Available with several reflector and light distribution options.;min. 80;E;1
PLEIAD G4 168 SURF DALI WHITE WIDE HL 830_72635-402;0.5;3000;3816;Aluminium - Fagerhult - White;3816;3000;3000;20;154;143;While;Aluminium - Fagerhult - White;7320047803260;72635-402;27;27;168;Pleiad G4 168 Surface mounted;Surface mounted installation. Installation section with two securing holes. See accessories for suspended installation.;Surface mounted downlights with integrated option for surface-mounted cable. Available with several reflector and light distribution options.;min. 80;E;1
PLEIAD G4 168 SURF DALI WHITE WIDE HL 840_72637-402;0.5;4000;3910;Aluminium - Fagerhult - White;3910;4000;4000;20;154;146;While;Aluminium - Fagerhult - White;7320047803345;72637-402;27;27;168;Pleiad G4 168 Surface mounted;Surface mounted installation. Installation section with two securing holes. See accessories for suspended installation.;Surface mounted downlights with integrated option for surface-mounted cable. Available with several reflector and light distribution options.;min. 80;E;1
PLEIAD G4 168 SURF DALI BLACK WIDE HL 830_72665-20728;0.5;3000;3076;Aluminium - Fagerhult - Black;3076;3000;3000;20;154;115;Black;Aluminium - Fagerhult - Black;7320048606303;72665-20728;27;27;168;Pleiad G4 168 Surface mounted;Surface mounted installation. Installation section with two securing holes. See accessories for suspended installation.;Surface mounted downlights with integrated option for surface-mounted cable. Available with several reflector and light distribution options.;min. 80;E;1
PLEIAD G4 168 SURF DALI BLACK WIDE HL 840_72665-20734;0.5;4000;3151;Aluminium - Fagerhult - Black;3151;4000;4000;20;154;118;Black;Aluminium - Fagerhult - Black;7320048766588;72665-20734;27;27;168;Pleiad G4 168 Surface mounted;Surface mounted installation. Installation section with two securing holes. See accessories for suspended installation.;Surface mounted downlights with integrated option for surface-mounted cable. Available with several reflector and light distribution options.;min. 80;E;1
