;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
RONDO G3 RECESSED WALLWASHER LL 840 CLO_308016;2.300;4000;1250;1250;4000;4000;66;147;89;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558726;308016;14;14;220;Rondo G3 recessed Wallwasher;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 RECESSED WALLWASHER LL 830 CLO_308012-402;2.300;3000;1163;1163;3000;3000;66;147;82;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558627;308012-402;14;14;220;Rondo G3 recessed Wallwasher;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 RECESSED WALLWASHER ML 830 CLO_308013;2.300;3000;2264;2264;3000;3000;66;147;79;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558641;308013;29;29;220;Rondo G3 recessed Wallwasher;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 RECESSED WALLWASHER ML 830 CLO_308013-402;2.300;3000;2264;2264;3000;3000;66;147;76;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558665;308013-402;30;30;220;Rondo G3 recessed Wallwasher;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 RECESSED WALLWASHER LL 840 CLO_308016-402;2.300;4000;1250;1250;4000;4000;66;147;89;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558740;308016-402;14;14;220;Rondo G3 recessed Wallwasher;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 RECESSED WALLWASHER ML 840 CLO_308017;2.300;4000;2434;2434;4000;4000;66;147;85;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558764;308017;29;29;220;Rondo G3 recessed Wallwasher;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 RECESSED WALLWASHER ML 840 CLO_308017-402;2.300;4000;2434;2434;4000;4000;66;147;82;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558788;308017-402;30;30;220;Rondo G3 recessed Wallwasher;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 RECESSED WALLWASHER LL 830 CLO_308012;2.300;3000;1163;1163;3000;3000;66;147;82;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558603;308012;14;14;220;Rondo G3 recessed Wallwasher;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
