;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
RONDO G3 RECESSED WIDE LL 830 CLO_308000-402;2.300;3000;1134;1134;3000;3000;66;147;119;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558146;308000-402;9.5;9.5;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE ML 830 CLO_308001;2.300;3000;2269;2269;3000;3000;66;147;125;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558160;308001;18;18;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE ML 830 CLO_308001-402;2.300;3000;2269;2269;3000;3000;66;147;121;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558184;308001-402;19;19;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE HL 830 CLO_308002;2.300;3000;3488;3488;3000;3000;66;147;115;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558207;308002;30;30;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE HL 830 CLO_308002-402;2.300;3000;3488;3488;3000;3000;66;147;111;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559518;308002-402;31;31;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE LL 840 CLO_308003;2.300;4000;1220;1220;4000;4000;66;147;128;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558245;308003;9.5;9.5;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE LL 840 CLO_308003-402;2.300;4000;1220;1220;4000;4000;66;147;128;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558269;308003-402;9.5;9.5;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE ML 840 CLO_308004;2.300;4000;2439;2439;4000;4000;66;147;134;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558283;308004;18;18;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE ML 840 CLO_308004-402;2.300;4000;2439;2439;4000;4000;66;147;130;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558306;308004-402;19;19;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE HL 840 CLO_308005;2.300;3000;3751;3751;3000;3000;66;147;124;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558320;308005;30;30;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE HL 840 CLO_308005-402;2.300;4000;3751;3751;4000;4000;66;147;119;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558344;308005-402;31;31;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM LL 830 CLO_308006;2.300;3000;1163;1163;3000;3000;66;147;122;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558368;308006;9.5;9.5;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM LL 830 CLO_308006-402;2.300;3000;1163;1163;3000;3000;66;147;122;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558382;308006-402;9.5;9.5;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM ML 830 CLO_308007;2.300;3000;2325;2325;3000;3000;66;147;128;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558405;308007;19;19;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM ML 830 CLO_308007-402;2.300;3000;2325;2325;3000;3000;66;147;124;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558429;308007-402;19;19;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM HL 830 CLO_308008;2.300;3000;3575;3575;3000;3000;66;147;118;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558443;308008;30;30;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM HL 830 CLO_308008-402;2.300;3000;3575;3575;3000;3000;66;147;114;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558467;308008-402;31;31;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM LL 840 CLO_308009;2.300;4000;1250;1250;4000;4000;66;147;132;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558481;308009;9.5;9.5;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM LL 840 CLO_308009-402;2.300;4000;1250;1250;4000;4000;66;147;132;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558504;308009-402;9.5;9.5;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM ML 840 CLO_308010;2.300;4000;2500;2500;4000;4000;66;147;137;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558528;308010;18;18;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM ML 840 CLO_308010-402;2.300;4000;2500;2500;4000;4000;66;147;134;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558542;308010-402;19;19;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM HL 840 CLO_308011;2.300;4000;3844;3844;4000;4000;66;147;127;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558566;308011;30;30;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED MEDIUM HL 840 CLO_308011-402;2.300;4000;3844;3844;4000;4000;66;147;122;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558580;308011-402;31;31;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 RECESSED WIDE LL 830 CLO_308000;2.300;3000;1134;1134;3000;3000;66;147;119;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558122;308000;9.5;9.5;220;Rondo G3 recessed;Luminaire for recessed ceiling installation, for ceiling thickness 5–50 mm. Stable assembly springs included. Hole pattern dimension: Ø 210 mm.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
