;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
RONDO G3 CEILING WALLWASHER LL 830 CLO_308030-402;3.400;3000;1163;1163;3000;3000;66;189;82;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559303;308030-402;14;14;193;Rondo G3 surface mounted Wallwasher;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 CEILING WALLWASHER ML 830 CLO_308031;3.400;3000;2264;2264;3000;3000;66;189;79;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559327;308031;29;29;193;Rondo G3 surface mounted Wallwasher;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 CEILING WALLWASHER ML 830 CLO_308031-402;3.400;3000;2264;2264;3000;3000;66;189;76;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559341;308031-402;30;30;193;Rondo G3 surface mounted Wallwasher;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 CEILING WALLWASHER LL 840 CLO_308032;3.400;4000;1250;1250;4000;4000;66;189;89;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559662;308032;14;14;193;Rondo G3 surface mounted Wallwasher;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 CEILING WALLWASHER LL 840 CLO_308032-402;3.400;4000;1250;1250;4000;4000;66;189;89;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559679;308032-402;14;14;193;Rondo G3 surface mounted Wallwasher;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 CEILING WALLWASHER ML 840 CLO_308033;3.400;4000;2434;2434;4000;4000;66;189;85;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559686;308033;29;29;193;Rondo G3 surface mounted Wallwasher;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 CEILING WALLWASHER ML 840 CLO_308033-402;3.400;4000;2434;2434;4000;4000;66;189;82;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559693;308033-402;30;30;193;Rondo G3 surface mounted Wallwasher;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
RONDO G3 CEILING WALLWASHER LL 830 CLO_308030;3.400;3000;1163;1163;3000;3000;66;189;82;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559280;308030;14;14;193;Rondo G3 surface mounted Wallwasher;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient robust downlight with several luminous fluxes.;min. 80;E;1
