;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
RONDO G3 CEILING WIDE LL 830 CLO_308018-402;3.400;3000;1134;1134;3000;3000;66;189;119;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558825;308018-402;9.5;9.5;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE LL 830 CLO_308018;3.400;3000;1134;1134;3000;3000;66;189;119;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558801;308018;9.5;9.5;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE ML 830 CLO_308019;3.400;3000;2269;2269;3000;3000;66;189;125;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558849;308019;18;18;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE ML 830 CLO_308019-402;3.400;3000;2269;2269;3000;3000;66;189;121;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558863;308019-402;19;19;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE HL 830 CLO_308020;3.400;3000;3488;3488;3000;3000;66;189;115;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558887;308020;30;30;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE HL 830 CLO_308020-402;3.400;3000;3488;3488;3000;3000;66;189;111;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558900;308020-402;31;31;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE LL 840 CLO_308021;3.400;4000;1220;1220;4000;4000;66;189;128;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558924;308021;9.5;9.5;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE LL 840 CLO_308021-402;3.400;4000;1220;1220;4000;4000;66;189;128;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558948;308021-402;9.5;9.5;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE ML 840 CLO_308022;3.400;4000;2439;2439;4000;4000;66;189;134;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558962;308022;18;18;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE ML 840 CLO_308022-402;3.400;4000;2439;2439;4000;4000;66;189;130;Anthracite;Aluminium - Fagerhult - Anthracite;7320047558986;308022-402;19;19;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE HL 840 CLO_308023;3.400;4000;3751;3751;4000;4000;66;189;124;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559006;308023;30;30;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING WIDE HL 840 CLO_308023-402;3.400;4000;3751;3751;4000;4000;66;189;119;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559020;308023-402;31;31;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM LL 830 CLO_308024;3.400;3000;1163;1163;3000;3000;66;189;122;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559044;308024;9.5;9.5;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM LL 830 CLO_308024-402;3.400;3000;1163;1163;3000;3000;66;189;122;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559068;308024-402;9.5;9.5;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM ML 830 CLO_308025;3.400;3000;2325;2325;3000;3000;66;189;128;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559082;308025;19;19;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM ML 830 CLO_308025-402;3.400;3000;2325;2325;3000;3000;66;189;124;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559105;308025-402;19;19;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM HL 830 CLO_308026;3.400;3000;3575;3575;3000;3000;66;189;118;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559129;308026;30;30;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM HL 830 CLO_308026-402;3.400;3000;3575;3575;3000;3000;66;189;114;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559143;308026-402;31;31;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM LL 840 CLO_308027;3.400;4000;1250;1250;4000;4000;66;189;132;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559167;308027;9.5;9.5;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM LL 840 CLO_308027-402;3.400;4000;1250;1250;4000;4000;66;189;132;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559181;308027-402;9.5;9.5;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM ML 840 CLO_308028;3.400;4000;2500;2500;4000;4000;66;189;137;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559204;308028;18;18;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM ML 840 CLO_308028-402;3.400;4000;2500;2500;4000;4000;66;189;134;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559228;308028-402;19;19;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM HL 840 CLO_308029;3.400;4000;3844;3844;4000;4000;66;189;127;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559242;308029;30;30;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
RONDO G3 CEILING MEDIUM HL 840 CLO_308029-402;3.400;4000;3844;3844;4000;4000;66;189;122;Anthracite;Aluminium - Fagerhult - Anthracite;7320047559266;308029-402;31;31;193;Rondo G3 surface mounted;Luminaire for ceiling installation. Ceiling bracket with bayonet fitting on 2 levels. Connection from above or via a surface-mounted cable in 3 possible directions.;Efficient, robust downlight suitable for various application areas with several luminous fluxes and distribution angles.;min. 80;E;1
