";Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Size##OTHER##"
"GLOBIA CLASSIC CEIL D450/170 LL 830 GLASS GLOBE_59150-20020;6;3000;3226;Glass - Fagerhult - Opal;3226;3000;3000;20;600;112;Black;Steel sheet - Fagerhult - Black;7316911150301;59150-20020;28;28;450;Globia Classic;Two-point suspension c.t.c 70 mm or track assembly in Control track.;A round beam decorative luminaire in three sizes for entrances and stairwells, for example.;min. 80;C;1;3"
"GLOBIA CLASSIC CEIL D450/170 HL 840 GLASS GLOBE_59150-20025;6;4000;6093;Glass - Fagerhult - Opal;6093;4000;4000;20;600;132;White;Steel sheet - Fagerhult - White;7316911150424;59150-20025;47;47;450;Globia Classic;Two-point suspension c.t.c 70 mm or track assembly in Control track.;A round beam decorative luminaire in three sizes for entrances and stairwells, for example.;min. 80;C;1;3"
"GLOBIA CLASSIC CEIL D400/150 LL 830 ACRYLIC GLOBE_59150-20034;2.7;3000;3208;Acrylic - Fagerhult - Opal;3208;3000;3000;20;550;151;Black;Steel sheet - Fagerhult - Black;7316911831439;59150-20034;22;22;400;Globia Classic;Two-point suspension c.t.c 70 mm or track assembly in Control track.;A round beam decorative luminaire in three sizes for entrances and stairwells, for example.;min. 80;C;1;2"
"GLOBIA CLASSIC CEIL D450/170 HL 830 ACRYLIC GLOBE_59150-20032;4.8;3000;6093;Acrylic - Fagerhult - Opal;6093;3000;3000;20;600;127;White;Steel sheet - Fagerhult - White;7316911831507;59150-20032;47;47;450;Globia Classic;Two-point suspension c.t.c 70 mm or track assembly in Control track.;A round beam decorative luminaire in three sizes for entrances and stairwells, for example.;min. 80;C;1;3"
