;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##
DISCOVERY 1800 LM 3K EMERGENCY SELFTEST AT4 DALI 3H_57754;2.000;3000;1907;Polycarbonate - Fagerhult - Opal;1907;3000;3000;44;94;110;White;Polycarbonate - Fagerhult - White;7320046348076;57754;18;18;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1100 LM 3K_57750;1.600;3000;1181;Polycarbonate - Fagerhult - Opal;1181;3000;3000;44;94;133;White;Polycarbonate - Fagerhult - White;7320046348045;57750;9;9;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1100 LM 3K_57750-515;1.600;3000;1181;Polycarbonate - Fagerhult - Opal;1181;3000;3000;20;94;123;White;Polycarbonate - Fagerhult - White;7320046689346;57750-515;10;10;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;2
DISCOVERY 1100 LM 3K_57750-469;1.600;3000;1181;Polycarbonate - Fagerhult - Opal;1181;3000;3000;44;94;117;White;Polycarbonate - Fagerhult - White;7320046348267;57750-469;10;10;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1100 LM 4K_57751;1.600;4000;1215;Polycarbonate - Fagerhult - Opal;1215;4000;4000;44;94;137;White;Polycarbonate - Fagerhult - White;7320046348052;57751;9;9;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1100 LM 4K_57751-515;1.600;4000;1215;Polycarbonate - Fagerhult - Opal;1215;4000;4000;20;94;127;White;Polycarbonate - Fagerhult - White;7320046689360;57751-515;10;10;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;2
DISCOVERY 1100 LM 4K_57751-469;1.600;4000;1215;Polycarbonate - Fagerhult - Opal;1215;4000;4000;44;94;120;White;Polycarbonate - Fagerhult - White;7320046348281;57751-469;10;10;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 3K_57752;1.600;3000;1907;Polycarbonate - Fagerhult - Opal;1907;3000;3000;44;94;133;White;Polycarbonate - Fagerhult - White;7320046348069;57752;14;14;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 3K_57752-515;1.600;3000;1907;Polycarbonate - Fagerhult - Opal;1907;3000;3000;20;94;127;White;Polycarbonate - Fagerhult - White;7320046689377;57752-515;15;15;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;2
DISCOVERY 1800 LM 3K_57752-402;1.600;3000;1907;Polycarbonate - Fagerhult - Opal;1907;3000;3000;44;94;143;White;Polycarbonate - Fagerhult - White;7320046348311;57752-402;14.5;14.5;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 3K_57752-469;1.600;3000;1907;Polycarbonate - Fagerhult - Opal;1907;3000;3000;44;94;123;White;Polycarbonate - Fagerhult - White;7320046348328;57752-469;16;16;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 3K_57752-495;1.600;3000;1907;Polycarbonate - Fagerhult - Opal;1907;3000;3000;44;94;136;White;Polycarbonate - Fagerhult - White;7320046348342;57752-495;14.5;14.5;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 4K_57755;1.600;4000;1962;Polycarbonate - Fagerhult - Opal;1962;4000;4000;44;94;137;White;Polycarbonate - Fagerhult - White;7320046348083;57755;14;14;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 4K_57755-515;1.600;4000;1962;Polycarbonate - Fagerhult - Opal;1962;4000;4000;20;94;130;White;Polycarbonate - Fagerhult - White;7320046689384;57755-515;15;15;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;2
DISCOVERY 1800 LM 4K_57755-402;1.600;4000;1962;Polycarbonate - Fagerhult - Opal;1962;4000;4000;44;94;148;White;Polycarbonate - Fagerhult - White;7320046348397;57755-402;14.5;14.5;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 4K_57755-469;1.600;4000;1962;Polycarbonate - Fagerhult - Opal;1962;4000;4000;44;94;126;White;Polycarbonate - Fagerhult - White;7320046348403;57755-469;16;16;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 4K_57755-495;1.600;4000;1962;Polycarbonate - Fagerhult - Opal;1962;4000;4000;44;94;140;White;Polycarbonate - Fagerhult - White;7320046348427;57755-495;14.5;14.5;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 4K EMERGENCY SELFTEST AT4 DALI 3H_57757;2.000;4000;1962;Polycarbonate - Fagerhult - Opal;1962;4000;4000;44;94;107;White;Polycarbonate - Fagerhult - White;7320046348090;57757;18;18;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 3K_57758;1.600;3000;2578;Polycarbonate - Fagerhult - Opal;2578;3000;3000;44;94;142;White;Polycarbonate - Fagerhult - White;7320046348106;57758;18;18;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 3K_57758-515;1.600;3000;2578;Polycarbonate - Fagerhult - Opal;2578;3000;3000;20;94;137;White;Polycarbonate - Fagerhult - White;7320046689391;57758-515;18;18;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;2
DISCOVERY 2500 LM 3K_57758-402;1.600;3000;2578;Polycarbonate - Fagerhult - Opal;2578;3000;3000;44;94;142;White;Polycarbonate - Fagerhult - White;7320046396763;57758-402;19;19;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 3K_57758-469;1.600;3000;2578;Polycarbonate - Fagerhult - Opal;2578;3000;3000;44;94;134;White;Polycarbonate - Fagerhult - White;7320046396787;57758-469;19;19;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 3K_57758-495;1.600;3000;2578;Polycarbonate - Fagerhult - Opal;2578;3000;3000;44;94;137;White;Polycarbonate - Fagerhult - White;7320046396794;57758-495;19.5;19.5;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 4K_57759;1.600;4000;2652;Polycarbonate - Fagerhult - Opal;2652;4000;4000;44;94;147;White;Polycarbonate - Fagerhult - White;7320046348113;57759;18;18;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 4K_57759-515;1.600;4000;2652;Polycarbonate - Fagerhult - Opal;2652;4000;4000;20;94;141;White;Polycarbonate - Fagerhult - White;7320046689407;57759-515;18;18;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;2
DISCOVERY 2500 LM 4K_57759-402;1.600;4000;2652;Polycarbonate - Fagerhult - Opal;2652;4000;4000;44;94;147;White;Polycarbonate - Fagerhult - White;7320046396862;57759-402;19;19;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 4K_57759-469;1.600;4000;2652;Polycarbonate - Fagerhult - Opal;2652;4000;4000;44;94;137;White;Polycarbonate - Fagerhult - White;7320046396879;57759-469;19;19;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 4K_57759-495;1.600;4000;2652;Polycarbonate - Fagerhult - Opal;2652;4000;4000;44;94;141;White;Polycarbonate - Fagerhult - White;7320046396893;57759-495;19.5;19.5;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 3K EMERGENCY SELFTEST AT4 DALI 3H_57760;2.000;3000;2578;Polycarbonate - Fagerhult - Opal;2578;3000;3000;44;94;119;White;Polycarbonate - Fagerhult - White;7320046348120;57760;22;22;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 4K EMERGENCY SELFTEST AT4 DALI 3H_57761;2.000;4000;2652;Polycarbonate - Fagerhult - Opal;2652;4000;4000;44;94;123;White;Polycarbonate - Fagerhult - White;7320046348205;57761;22;22;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1100 LM 3K_57750-402;1.600;3000;1181;Polycarbonate - Fagerhult - Opal;1181;3000;3000;44;94;142;White;Polycarbonate - Fagerhult - White;7320046728373;57750-402;8.5;8.5;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1100 LM 3K_57750-533;1.600;3000;1181;Polycarbonate - Fagerhult - Opal;1181;3000;3000;20;94;123;White;Polycarbonate - Fagerhult - White;7316910348877;57750-533;10;10;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;3
DISCOVERY 1100 LM 4K_57751-533;1.600;4000;1215;Polycarbonate - Fagerhult - Opal;1215;4000;4000;20;94;127;White;Polycarbonate - Fagerhult - White;7316910348884;57751-533;10;10;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;3
DISCOVERY 1800 LM 3K_57752-533;1.600;3000;1907;Polycarbonate - Fagerhult - Opal;1907;3000;3000;20;94;135;White;Polycarbonate - Fagerhult - White;7320049860926;57752-533;15;15;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;3
DISCOVERY 1800 LM 4K_57755-533;1.600;4000;1962;Polycarbonate - Fagerhult - Opal;1962;4000;4000;20;94;139;White;Polycarbonate - Fagerhult - White;7316910348860;57755-533;15;15;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;3
DISCOVERY 2500 LM 3K_57758-533;1.600;3000;2578;Polycarbonate - Fagerhult - Opal;2578;3000;3000;20;94;139;White;Polycarbonate - Fagerhult - White;7320049860872;57758-533;20;20;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;3
DISCOVERY 2500 LM 4K_57759-533;1.600;4000;2652;Polycarbonate - Fagerhult - Opal;2652;4000;4000;20;94;143;White;Polycarbonate - Fagerhult - White;7320049860889;57759-533;20;20;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;3
DISCOVERY 1800 LM 3K_57752-569;1.600;3000;1907;Polycarbonate - Fagerhult - Opal;1907;3000;3000;44;94;132;White;Polycarbonate - Fagerhult - White;7316910866548;57752-569;15;15;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 4K_57755-569;1.600;4000;1962;Polycarbonate - Fagerhult - Opal;1962;4000;4000;44;94;136;White;Polycarbonate - Fagerhult - White;7316910866555;57755-569;15;15;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 3K_57758-569;1.600;3000;2578;Polycarbonate - Fagerhult - Opal;2578;3000;3000;44;94;134;White;Polycarbonate - Fagerhult - White;7316910866562;57758-569;20;20;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 4K_57759-569;1.600;4000;2652;Polycarbonate - Fagerhult - Opal;2652;4000;4000;44;94;138;White;Polycarbonate - Fagerhult - White;7316910866579;57759-569;20;20;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 3K_57752-581;1.600;3000;1907;Polycarbonate - Fagerhult - Opal;1907;3000;3000;44;94;132;White;Polycarbonate - Fagerhult - White;7316912983427;57752-581;15;15;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 1800 LM 4K_57755-581;1.600;4000;1962;Polycarbonate - Fagerhult - Opal;1962;4000;4000;44;94;136;White;Polycarbonate - Fagerhult - White;7316912983441;57755-581;15;15;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 3K_57758-581;1.600;3000;2578;Polycarbonate - Fagerhult - Opal;2578;3000;3000;44;94;134;White;Polycarbonate - Fagerhult - White;7316912983465;57758-581;20;20;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
DISCOVERY 2500 LM 4K_57759-581;1.600;4000;2652;Polycarbonate - Fagerhult - Opal;2652;4000;4000;44;94;138;White;Polycarbonate - Fagerhult - White;7316912983489;57759-581;20;20;359;Discovery;Four securing holes. For recess or surface mounting on ceilings or walls. Brackets for recessed installation ordered separately, please see accessories. There are holes for a surface mounted installation socket. <br>The luminaire must not be covered with insulation. For further details please refer to the assembly instructions.</br>;"ISCC-certified all-round luminaire in plastic based on renewable materials instead of fossil oil with IP 44 that satisfies needs in more demanding environments.
An elegant design with high efficiency that gives a space-creating lighting pattern for stairwells, corridors, kitchens, bathrooms and cellars.";min. 80;C;1;1
