;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Installation##OTHER##;Lighting Control##OTHER##;LightDistribution##OTHER##
NOTOR36 TRACK D 600 DALI HL OPAL 830_16088-20010;36;0.7;3000;1400;Acrylic - Fagerhult - Opal;612;20;81;95;White;Aluminium - Fagerhult - White;7316910002045;16088-20010;15.5;Notor 36 Track Opal;In Lighting Track Pro (on/off), Control Track or Control Track Dual (DALI). Adapter locks mechanically to the rail with a knob.;Luminaire for installation on lighting tracks with Opal louvre.;min. 80;C;1;1;0;Notor-36-Track-Opal : 16088-20010
NOTOR36 TRACK D 1200 DALI HL OPAL 830_16088-20003;36;1.4;3000;2800;Acrylic - Fagerhult - Opal;1250;20;81;105;White;Aluminium - Fagerhult - White;7316910001925;16088-20003;28.5;Notor 36 Track Opal;In Lighting Track Pro (on/off), Control Track or Control Track Dual (DALI). Adapter locks mechanically to the rail with a knob.;Luminaire for installation on lighting tracks with Opal louvre.;min. 80;E;1;1;0;Notor-36-Track-Opal : 16088-20003
NOTOR36 TRACK D 1200 CAS LL OPAL 830_16088-20006;36;1.4;3000;1800;Acrylic - Fagerhult - Opal;1250;20;81;103;White;Aluminium - Fagerhult - White;7316910001963;16088-20006;18;Notor 36 Track Opal;In Lighting Track Pro (on/off), Control Track or Control Track Dual (DALI). Adapter locks mechanically to the rail with a knob.;Luminaire for installation on lighting tracks with Opal louvre.;min. 80;E;1;2;0;Notor-36-Track-Opal : 16088-20006
NOTOR36 TRACK D 600 CAS LL OPAL 830_16088-20012;36;0.7;3000;900;Acrylic - Fagerhult - Opal;612;20;81;90;White;Aluminium - Fagerhult - White;7316910002083;16088-20012;10.5;Notor 36 Track Opal;In Lighting Track Pro (on/off), Control Track or Control Track Dual (DALI). Adapter locks mechanically to the rail with a knob.;Luminaire for installation on lighting tracks with Opal louvre.;min. 80;C;1;2;0;Notor-36-Track-Opal : 16088-20012
NOTOR36 TRACK D 1200 OR HL OPAL 830_16088-20062;36;1.5;3000;2800;Acrylic - Fagerhult - Opal;1326;20;67;110;White;Aluminium - Fagerhult - White;7316911826336;16088-20062;27;Notor 36 Track Opal;In Lighting Track Pro (on/off), Control Track or Control Track Dual (DALI). Adapter locks mechanically to the rail with a knob.;Luminaire for installation on lighting tracks with Opal louvre.;min. 80;C;1;3;1;Notor-36-Track-Opal : 16088-20062
