;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Light_Distribution##OTHER##;Reflector_type##OTHER##
STREAMER X SPOTLIGHT NARROW STD HL 930_80278-20000;85;0.5;3000;3210;Aluminium - Fagerhult - Specular;162;20;153;136;White;Aluminium - Fagerhult - White;7316913014809;80278-20000;24;85;Streamer X;"Luminaire for installation in Lighting Track Pro (on/off, Casambi or OR) 3-phase track, or Control Track Dual (DALI).
The adapter locks mechanically to the track with a knob. Phase 1, 2 or 3 can then be selected with the phase selector knob.
For detailed information, see the installation instructions.";Streamer X is an efficient and dynamic track-mounted spotlight for indoor applications. A newly developed modular solution enables an easy replacement of the LED module when needed, providing increased flexibility and long-term durability.;min. 90;D;1;Light_Streamer_X : 80278-20000;1
STREAMER X SPOTLIGHT MEDIUM STD HL 930_80278-20001;85;0.5;3000;3187;Aluminium - Fagerhult - Specular;162;20;153;135;White;Aluminium - Fagerhult - White;7316913014830;80278-20001;24;85;Streamer X;"Luminaire for installation in Lighting Track Pro (on/off, Casambi or OR) 3-phase track, or Control Track Dual (DALI).
The adapter locks mechanically to the track with a knob. Phase 1, 2 or 3 can then be selected with the phase selector knob.
For detailed information, see the installation instructions.";Streamer X is an efficient and dynamic track-mounted spotlight for indoor applications. A newly developed modular solution enables an easy replacement of the LED module when needed, providing increased flexibility and long-term durability.;min. 90;D;1;Light_Streamer_X : 80278-20001;1
STREAMER X SPOTLIGHT WIDE STD HL 930_80278-20002;85;0.5;3000;3180;Aluminium - Fagerhult - Specular;162;20;153;136;White;Aluminium - Fagerhult - White;7316913014861;80278-20002;24;85;Streamer X;"Luminaire for installation in Lighting Track Pro (on/off, Casambi or OR) 3-phase track, or Control Track Dual (DALI).
The adapter locks mechanically to the track with a knob. Phase 1, 2 or 3 can then be selected with the phase selector knob.
For detailed information, see the installation instructions.";Streamer X is an efficient and dynamic track-mounted spotlight for indoor applications. A newly developed modular solution enables an easy replacement of the LED module when needed, providing increased flexibility and long-term durability.;min. 90;D;1;Light_Streamer_X : 80278-20002;1
STREAMER X SPOTLIGHT EXTRA WIDE STD HL 930_80278-20003;85;0.5;3000;3205;Aluminium - Fagerhult - Specular;162;20;153;135;White;Aluminium - Fagerhult - White;7316913014892;80278-20003;24;85;Streamer X;"Luminaire for installation in Lighting Track Pro (on/off, Casambi or OR) 3-phase track, or Control Track Dual (DALI).
The adapter locks mechanically to the track with a knob. Phase 1, 2 or 3 can then be selected with the phase selector knob.
For detailed information, see the installation instructions.";Streamer X is an efficient and dynamic track-mounted spotlight for indoor applications. A newly developed modular solution enables an easy replacement of the LED module when needed, providing increased flexibility and long-term durability.;min. 90;D;1;Light_Streamer_X : 80278-20003;1
STREAMER X SPOTLIGHT WW STD HL 930_80278-20004;85;0.5;3000;3291;Aluminium - Fagerhult - Specular;162;20;153;139;White;Aluminium - Fagerhult - White;7316913014922;80278-20004;24;85;Streamer X;"Luminaire for installation in Lighting Track Pro (on/off, Casambi or OR) 3-phase track, or Control Track Dual (DALI).
The adapter locks mechanically to the track with a knob. Phase 1, 2 or 3 can then be selected with the phase selector knob.
For detailed information, see the installation instructions.";Streamer X is an efficient and dynamic track-mounted spotlight for indoor applications. A newly developed modular solution enables an easy replacement of the LED module when needed, providing increased flexibility and long-term durability.;min. 90;D;1;Light_Streamer_X : 80278-20004;2
